Dual Radars GUI setup:

1. Change mmWavePath in MATLAB appDesigner for dual\_radars\_gui
2. Check \functions\scripts\ .ps1 files to ensure mmWave path is correct
3. Copy DCAFile1.json and DCAFile2.json to mmWaveStudio\PostProc\
4. Make sure IP addresses are correct in Network Connections
5. Modify path to store data inside of DCAFileX.json files
6. Inside MATLAB app, make sure you are in the functions folder (should be automatic now)
7. Check comport label.png to know which port is which on the 6843